How to use Snap-Caps
The fixing is secured through the washer into the work piece. The cap is then "snapped" over the washer, mating by means of an interlocking peripheral groove and flange. This provides an airtight and seal that excludes atmosphere and protects the fastener head from rust and corrosion.
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